{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":24,"n_cols":34,"rows_kept":24,"merged":[[0,0,0,33],[1,0,1,3],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,2,32],[2,33,3,33],[18,0,18,3],[19,0,20,3],[19,4,20,5],[19,6,19,23],[19,24,19,26],[19,27,19,29],[19,30,19,32],[19,33,20,33],[20,6,20,8],[20,9,20,11],[20,12,20,14],[20,15,20,17],[20,18,20,20],[20,21,20,23],[20,24,20,26],[20,27,20,29],[20,30,20,32],[21,0,23,3],[21,6,21,8],[21,9,21,11],[21,12,21,14],[21,15,21,17],[21,18,21,20],[21,21,21,23],[21,24,21,26],[21,27,21,29],[21,30,21,32],[22,6,22,8],[22,9,22,11],[22,12,22,14],[22,15,22,17],[22,18,22,20],[22,21,22,23],[22,24,22,26],[22,27,22,29],[22,30,22,32],[23,4,23,5],[23,6,23,8],[23,9,23,11],[23,12,23,14],[23,15,23,17],[23,18,23,20],[23,21,23,23],[23,24,23,26],[23,27,23,29],[23,30,23,32]],"flags":["formulas_cached_only"]}
["宁波旭升集团股份有限公司减排计划及碳排路径"]
["一：减排计划"]
["序号","类别","排放源","现状","改善措施","减排量","年度别(具体时间节点)",{"$nulls":26},"备注"]
[{"$nulls":6},24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50]
["1","类别1","直接排放","熔炼炉在熔铝过程中,有铝锭熔化阶段和铝液保温阶段。合理安排工作计划减少保温耗气","对熔铝量进行计算选择对应的熔炼炉，使用过程中控制加料间隔，减少铝液保温时间","减排300T"]
["2",null,null,"叉车在搬运过程中存在较长时间未熄火等待现象","对运输车辆驾驶人员进行资料宣传教育，避免等待中浪费柴油","-"]
["3",null,null,"熔铝采用天然气燃烧,无法采用绿电/绿证进行碳排抵消","在碳排放交易CCER市场化成熟后,逐年加大交易占比","到2035年碳排交易40%，抵扣17070T;\n到2040年碳排交易85%，抵扣36290T；",{"$nulls":8},{"v":0.1,"d":"10%"},{"v":0.2,"d":"20%"},{"v":0.3,"d":"30%"},{"v":0.4,"d":"40%"},{"v":0.5,"d":"50%"},{"v":0.6,"d":"60%"},{"v":0.7,"d":"70%"},{"v":0.8,"d":"80%"},{"v":0.85,"d":"85%"},{"v":0.9,"d":"90%"},{"v":0.9,"d":"90%"},{"v":0.95,"d":"95%"},{"v":0.95,"d":"95%"},{"v":0.95,"d":"95%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"}]
["4","类别2","外购电力","绿电目前只采用在厂房屋顶上安装分布式光伏,5~7厂装机容量达到14.5MWp","从25开始逐年增加外购绿电或绿证,确保在35年到达100%使用绿电","到2030年外购绿电60%,减排29860T;\n到2035年外购绿电100%,减排49785T;",null,{"v":0.1,"d":"10%"},{"v":0.2,"d":"20%"},{"v":0.3,"d":"30%"},{"v":0.4,"d":"40%"},{"v":0.5,"d":"50%"},{"v":0.6,"d":"60%"},{"v":0.7,"d":"70%"},{"v":0.8,"d":"80%"},{"v":0.9,"d":"90%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"},{"v":1,"d":"100%"}]
["5",null,null,"日常照明用电管理不足","定期1次/2月进行照明用电管理，确保在利用自然光情况下不开灯或少开灯","-"]
["6",null,null,"车间局部供给压力过高，连接软管存在漏气现象","合理控制压缩空气供给压力减少电力使用\n1次/2月，漏气专项检查","减排330T"]
["7",null,null,"生产计划小批量多频次，造成能源浪费，碳排放量高","对计划进行调整，进行集中生产，减少能源损耗，提升效率","-"]
["8","类别3","运输排放","采用燃油货车送货","合理规划送货计划，短距离采用氢能源货车送货，提升环保降碳","-"]
["9",null,null,"供应商管理研究包装材料替代的可能性","包装材料尽可能采用可循环利用的材料","-"]
["10",null,"产品间接排放","绿铝相对原铝价格较高，还未采用绿铝","根据碳排实际逐年增加绿铝购买比例","5~7厂按各厂区需要比例购买\n到2030年，购买减排291060T；\n到2035年，购买减排476322T；",null,{"v":0.1,"d":"10%"},{"v":0.2,"d":"20%"},{"v":0.3,"d":"30%"},{"v":0.4,"d":"40%"},{"v":0.5,"d":"50%"},{"v":0.6,"d":"60%"},{"v":0.7,"d":"70%"},{"v":0.8,"d":"80%"},{"v":0.9,"d":"90%"},{"v":1,"d":"100%"}]
["11",null,null,"考虑回收铝对产品品质的影响还未采购","区别压铸、锻造、挤压工艺，对压铸产品逐年增加回收铝应用比例。","5、7厂压铸再生铝购买\n到2030年，购买减排128838T；\n到2035年，购买减排193260T；",null,null,{"v":0.1,"d":"10%"},{"v":0.1,"d":"10%"},{"v":0.1,"d":"10%"},{"v":0.2,"d":"20%"},{"v":0.2,"d":"20%"},{"v":0.2,"d":"20%"},{"v":0.3,"d":"30%"},{"v":0.3,"d":"30%"},{"v":0.3,"d":"30%"},{"v":0.3,"d":"30%"},{"v":0.3,"d":"30%"},{"v":0.4,"d":"40%"},{"v":0.4,"d":"40%"},{"v":0.4,"d":"40%"},{"v":0.4,"d":"40%"},{"v":0.4,"d":"40%"},{"v":0.4,"d":"40%"},{"v":0.4,"d":"40%"},{"v":0.4,"d":"40%"},{"v":0.4,"d":"40%"},{"v":0.4,"d":"40%"},{"v":0.4,"d":"40%"},{"v":0.4,"d":"40%"},{"v":0.4,"d":"40%"},{"v":0.4,"d":"40%"}]
["12",null,null,"除铝锭以外的原辅材及因工艺要求无法采用回收铝，需其他途径进行碳抵消","在碳排放交易CCER市场化成熟后,不足部分采用CCER碳抵消","到2035年，购买抵消123072T；\n到2040年，购买抵消203969T；",{"$nulls":8},{"v":0.1,"d":"10%"},{"v":0.2,"d":"20%"},{"v":0.3,"d":"30%"},{"v":0.4,"d":"40%"},{"v":0.5,"d":"50%"},{"v":0.5,"d":"50%"},{"v":0.7,"d":"70%"},{"v":0.7,"d":"70%"},{"v":0.75,"d":"75%"},{"v":0.75,"d":"75%"},{"v":0.8,"d":"80%"},{"v":0.8,"d":"80%"},{"v":0.85,"d":"85%"},{"v":0.85,"d":"85%"},{"v":0.9,"d":"90%"},{"v":0.9,"d":"90%"},{"v":0.9,"d":"90%"},{"v":0.95,"d":"95%"},{"v":0.95,"d":"95%"}]
["13",null,null,"操作工经验及设备性能等因素，产品合格率有提升空间","提高产品合格率，减少压铸过程及加工过程中脱模剂与切削液的使用量","合格率8%提升，可减少碳排1104T"]
[]
["二：碳排路径"]
["区分",{"$nulls":3},"碳排范围",null,"中长期碳排强度（t-CO2/t-Al）",{"$nulls":17},"2023-",null,null,"2023-",null,null,"2023-",null,null,"备注"]
[{"$nulls":6},2023,null,null,2030,null,null,2035,null,null,2040,null,null,2045,null,null,2050,null,null,2030,null,null,2040,null,null,2050]
["5厂、6厂、7厂含总部\n（压铸、锻造、挤压）",{"$nulls":3},"范围一+二","-",{"v":1.409,"d":"1.41"},null,null,{"v":0.975,"d":"0.98"},null,null,{"v":0.448,"d":"0.45"},null,null,{"v":0.174,"d":"0.17"},null,null,{"v":0.114,"d":"0.11"},null,null,0.07,null,null,{"v":-0.3080198722498226,"d":"-31%"},null,null,{"v":-0.8765081618168915,"d":"-88%"},null,null,{"v":-0.9503193754435769,"d":"-95%"}]
[{"$nulls":4},"范围三","-",{"v":13.917,"d":"13.92"},null,null,{"v":7.9,"d":"7.90"},null,null,{"v":2.6,"d":"2.60"},null,null,{"v":1,"d":"1.00"},null,null,{"v":0.6,"d":"0.60"},null,null,{"v":0.2,"d":"0.20"},null,null,{"v":-0.4323489257742329,"d":"-43%"},null,null,{"v":-0.928145433642308,"d":"-93%"},null,null,{"v":-0.9856290867284616,"d":"-99%"}]
[{"$nulls":4},"合计",null,{"v":15.326,"d":"15.33"},null,null,{"v":8.875,"d":"8.88"},null,null,{"v":3.048,"d":"3.05"},null,null,{"v":1.174,"d":"1.17"},null,null,{"v":0.714,"d":"0.71"},null,null,0.27,null,null,{"v":-0.4209187002479447,"d":"-42%"},null,null,{"v":-0.9233981469398408,"d":"-92%"},null,null,{"v":-0.9823828787681065,"d":"-98%"}]